;-------------------------------------------------------
; INF file for DS40xxHC/HCS/HC+/HF/HS/MD Series Driver 
; For Windows 2000/XP/2003/Vista(32-bit)
; Copyright (C) Hikvision Digital Technology Co.,Ltd.


[Version]
Signature="$WINDOWS NT$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%DS400XX%
DriverVer=05/04/2008,2.1.1.1


; ================= Device Install section =====================

[Manufacturer]
%Manufacturer%=DS400x

[ControlFlags]
ExcludeFromSelect=*

[DS400x]
%DS40XXHC.DeviceDesc% = DS40XXHC, PCI\VEN_104c&DEV_9065

[DestinationDirs]
DS40XXHC.CopyList  =  10,system32\drivers      ; WinXX\system32\drivers

[DS40XXHC]
CopyFiles=DS40XXHC.CopyList

[DS40XXHC.Services]
AddService = DS40XXHC,0x00000002,DS40XXHC.AddReg

[DS40XXHC.AddReg]
ServiceType   = 1	; KERNEL MODE DRIVER
StartType     = 3	; MANUAL
ErrorControl  = 1	; NORMAL
ServiceBinary = %12%\DS40xxDrv.sys

[DS40XXHC.CopyList]
DS40xxDrv.sys

[Strings]
DS400XX=     "Hangzhou Hikvision Digital Techinology Co.,Ltd."
Manufacturer="Hangzhou Hikvision Digital Techinology Co.,Ltd."
DS40XXHC.DeviceDesc="Hikvision DS40xxHC/HCS/HC+/HF/HS/MD Series"
DISKID="DS40xx serial card Installation Disk"



